

TECHNICAL SHEET

|  |  |
| --- | --- |
| **Designation** | **EARLOOP MASKS** |
| **References** | White | Blue | Green | Rose |
| 3135024 | 3135025 | 3135026 | 3135030 |
| **Product picture** | Une image contenant texte  Description générée automatiquement |
| **Product****description** | Medical Masks with elastics triple thickness without latex and without fiberglasses. In compliance with the Typical standard IIR IN 14683: protective masks **against the projections of biological liquids.** |
| **Characteristics and****composition** | * Bacterial Filtration Efficiency (BFE): >99%.
* Respiratory resistance (ΔP): < 49 Pa/cm².
* Splash resistance: > 120 mm Hg. Propreté microbienne (UFC/g) : ≤ 30
* Inner and top layer: Spunbound polypropylene
* Filter: Meltblown polypropylene
* Dimensions : 17,3 cm x 8,9 cm (± 0,3 cm).
* 3 ply
 |
| **Packaging** | 50 masks per box. 10 boxes per carton. |
| **Shelf life** | 3 years40°C |
| **Indications** **of use** | Une image contenant texte  Description générée automatiquement5°C |
| **Legal****information** | Medical device of class I under MDR 2017/745 RegulationEC Mark - Manufacturer A.R. MEDICOM INC. (Shanghai) Co., Ltd. |

Version 1.0 – 03/01/2024