

TECHNICAL SHEET

|  |  |
| --- | --- |
| **Designation** | **TIE-ON MASKS** |
| **Reference(s)** | Blue |
| 3135073 |
| **Product picture** |  |
| **Product description** | Medical tie-on masks, 3 plies, latex and fiberglass free. Complies with EN 14683 norm Type IIR. |
| **Characteristics and compositions** | Bacterial Filtration Efficiency (BFE): >99%.  • Respiratory resistance (ΔP): < 49 Pa/cm².  • Splash resistance: > 120 mm Hg.  • Dimensions: 8.9 cm x 17.8 cm.  • Integrated nose piece.  • 3 plies |
| **Packaging** | Box of 50 masks.  6 boxes per carton. |
| **Shelf life** | NA |
| **Indications of use** | Une image contenant texte  Description générée automatiquement  40°C  5°C |
| **Legal information** | Medical Device of class I under MDR 2017/745 regulation  EC Mark - Manufacturer A.R. MEDICOM INC. (Shanghai) Co., Ltd. |

Version 1.0 – 03/01/2024