

TECHNICAL SHEET

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Designation** | **EARLOOP MASKS** | | | |
| **References** | White | Blue | Green | Rose |
| 3135024 | 3135025 | 3135026 | 3135030 |
| **Product picture** | Une image contenant texte  Description générée automatiquement | | | |
| **Product**  **description** | Medical Masks with elastics triple thickness without latex and without fiberglasses. In compliance with the Typical standard IIR IN 14683: protective masks **against the projections of biological liquids.** | | | |
| **Characteristics and**  **composition** | * Bacterial Filtration Efficiency (BFE): >99%. * Respiratory resistance (ΔP): < 49 Pa/cm². * Splash resistance: > 120 mm Hg. Propreté microbienne (UFC/g) : ≤ 30 * Inner and top layer: Spunbound polypropylene * Filter: Meltblown polypropylene * Dimensions : 17,3 cm x 8,9 cm (± 0,3 cm). * 3 ply | | | |
| **Packaging** | 50 masks per box.  10 boxes per carton. | | | |
| **Shelf life** | 3 years  40°C | | | |
| **Indications**  **of use** | Une image contenant texte  Description générée automatiquement  5°C | | | |
| **Legal**  **information** | Medical device of class I under MDR 2017/745 Regulation  EC Mark - Manufacturer A.R. MEDICOM INC. (Shanghai) Co., Ltd. | | | |

Version 1.0 – 03/01/2024