

TECHNICAL SHEET

|  |  |
| --- | --- |
| **Product** | **Taper Round and Flat End** |
| **Reference** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Description** | C1 | C2 | F1R | F2R | F1 |
| **Code** | 855 | 855L | 850 | 850 | 848 |
| **ISO** | 014 | 018 | 016 | 018 | 016 |
| **LWP (mm)** | 6,3 | 7 | 10 | 10 | 10 |
| **TL (mm)** | 21 | 19 | 22,5 | 22,5 | 22,5 |
| **Ref. Coarse** | 3138066 | 3138067 | 3138447 | 3138068 | 3138065 |

 |
| **Picture** |  |
| **Product description** | Taper Round and Flat End burs. |
| **Characteristics** **& composition** | * Sterile burs for maximum hygiene: no risk of cross contamination.
* Sterilized by gamma radiation: ready to use!

 – Checked individually, controlled manufacturing guaranteed |
| **Packaging** | Box of 25 burs.  |
| **Shelf life** |  |
| **Legal information** | Class: IIA.CE Marking 0483. ICIM S.p.A Notified body. Manufacturer: STRAUSS & CO.. |

Version 2.2 created the 15/11/2022 by RG